[ES503]

기    능

본 기기는 다양한 환경에 대응하도록 구성이 가능한 컴팩트한 TRI-AMP 디지털 ACTIVE 스피커 시스템이다.  마스터 LF 12“와 슬레이브 HF 3"x4ea 스피커 2개를 탑온탑으로 쉽고 빠르게 연결하여 기본(싱글컬럼)세트로 구성하여 사용한다.

ES 엔터테인먼트 시스템은 3가지 시스템 운영타입(싱글컬럼/싱글스테레오/더블컬럼)으로 다양한 공간에 대응하며, 앰프모듈에 사용자 친화적인 OLED디스플레이가 있어, 직관적으로 손쉽게 설정 할 수 있다.

토탈 인풋 5채널의 온보드 디지털믹서가 있으며, 기본 장착된 블루투스 오디오 리시버는 모바일 기기에서의 무선입력을 허용하여 컴팩트하고 다양한 환경에 대응하는 컴팩트하고 강력한 시스템이다.

사    양

Technical Data

Speaker Type : 3-amped Stereo System with two full-range tops and one subwoofer

Acoustical data

Frequency Response [-10dB]	: 37 - 15.000 Hz

Max SPL	: 121 dB

MF – HF	: 8x 3"

Type MF – HF	: Neodymium

LF	: 12"

Directivity	: 95x65°

Amplifier

Amp Technology	: Digipro® G3

Amp Class	: Class-D

Power Amp	: 1000 W

Power Supply	: SMPS with PSU Auto-range

Power Connection	: VDE socket

Cooling	: Convection

Controls	: 1x OLED Display with rotary encoder	w/switch 1x Audio signal monitoring LED 1x	USB port (service data)

Processor

Controller	: DSP 24 Bit/48 kHz

System Presets	: Factory presets + User defined

Limiter	: Dual Active, Peak, RMS, Thermal

Crossover Frequency LF-HF	: 206 Hz

Input

Mic/Instrument Channel	: 1x Combo (XLR/Jack) balanced/unbalanced	input

Line Channels	: 2x Combo (XLR/Jack) balanced/unbalanced	inputs

Media Channel	: 1x Bluetooth® built-in receiver

Mix Output	: 1x XLR balanced output

Mechanics

Housing (Subwoofer)	: 15mm Black Painted Birch Plywood

Housing (Tops)	: Polypropylene PP

Handles	: 2x lateral side (Subwoofer)

Width (Top)	: 95 mm (3.74 in)

Height (Top)	: 360 mm (13.98 in)

Depth (Top)	: 137 mm (5.39 in)

Width (Subwoofer)	: 465 mm (18.3 in)

Height (Subwoofer)	: 400 mm (15.7 in)

Depth (Subwoofer)	: 430 mm (16.9 in)

Weight (Top)	: 1.9Kg – 4.19lbs.

Weight (Subwoofer)	: 16.4Kg – 36.16lbs.

※ 상기 사양 및 동등 이상품 이어야한다